{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["507142"],"not_rendered":{"charts":0,"images":3,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"507142","index":0,"n_rows":26,"n_cols":10,"rows_kept":26,"cut":false,"hidden":false,"merged":[[1,1,1,10],[0,1,0,10],[3,1,3,10],[2,1,2,10],[9,0,9,1]],"flags":["formulas_cached_only"]}
[null,"Raccordi a tenuta frontale O.R."]
[null,"Connectors o-ring face seal"]
[null,"507142 - Terminale orientabile 90°  femmina ORFS - GAS cil. (BSPP)  con O.R. e rondella  per sedi ISO 1179"]
[null,"507142 - 90° (ADJ) elbow swivel nut  ORFS - male BSPP  with O.R. and retaining ring  ISO 1179 ports"]
[]
[]
[]
[]
[]
["T","T","REFERENCE","F","F1","B","C","CH","CH1","HasCadenas"]
["mm","in"]
["6","1/4","A507142-0610","9/16-18 UNF-2A","G1/8-28 A GAS","34,5","30","14","17","True"]
["6","1/4","A507142-0613","9/16-18 UNF-2A","G1/4-19 A GAS","34,5","35","19","17","True"]
["8-10","5/16-3/8","A507142-1013","11/16-16 UN-2A","G1/4-19 A GAS","40","36","19","22","True"]
["8-10","5/16-3/8","A507142-1017","11/16-16 UN-2A","G3/8-19 A GAS","40","38","22","22","True"]
["12","1/2","A507142-1217","13/16-16 UN-2A","G3/8-19 A GAS","48","40,5","22","24","True"]
["12","1/2","A507142-1221","13/16-16 UN-2A","G1/2-14 A GAS","48","48","27","24","True"]
["14÷16","5/8","A507142-1621","1\"-14 UNS-2A","G1/2-14 A GAS","54","48","27","30","True"]
["14÷16","5/8","A507142-1626","1\"-14 UNS-2A","G3/4-14 A GAS","55","51,5","36","30","True"]
["18-20","3/4","A507142-2026","1\"3/16-12 UN-2A","G3/4-14 A GAS","59,5","51,5","36","36","True"]
["18-20","3/4","A507142-2033","1\"3/16-12 UN-2A","G1\"-11 A GAS","61","58","41","36","True"]
["22-25","7/8-1\"","A507142-2533","1\"7/16-12 UN-2A","G1\"-11 A GAS","65","58","41","41","True"]
["22-25","7/8-1\"","A507142-2542","1\"7/16-12 UN-2A","G1\"1/4-11 A GAS","67","60,5","50","41","True"]
["28÷32","1\"1/4","A507142-3242","1\"11/16-12 UN-2A","G1\"1/4-11 A GAS","67,5","60,5","50","50","True"]
["28÷32","1\"1/4","A507142-3248","1\"11/16-12 UN-2A","G1\"1/2-11 A GAS","70,5","64,5","60","50","True"]
["35-38","1\"1/2","A507142-3848","2\"-12 UN-2A","G1\"1/2-11 A GAS","74","64,5","60","57","False"]